**Even more reach now available in demolition: SENNEBOGEN 870 E: 36 m long front demolition excavator**

**The 870 E demolition material handler, introduced by SENNEBOGEN at the end of 2017, is a uniquely special machine that can be called into action when high levels of reach and precision are required for the demolition of buildings and industrial plants. SENNEBOGEN are now offering their customers, ex works, the 870 E with the original 33 m long attachment or, alternatively, featuring a longer 36 m version with a working load of 4 t.**

The new, longer attachment consists of a 19.5 m basic boom with a quick-change facility and a 2.5 m intermediate boom, along with the 12.5 m stick with reversing mechanism. This gives the equipment an overall vertical reach of 36 m and a boom range of 20 m. The demolition excavator can handle loads of up to 4 t with ease across the entire working range. 33 m long equipment is also available.

SENNEBOGEN has shown once again that it can successfully integrate customer-specific requirements into its range. This machine will be presented to the general public for the first time at bauma. Special focus is also afforded to the particularly stable construction of the machine and the extremely robust finishing of all the components. Visitors to the trade fair in Munich from April 8, 2019 can check it out for themselves.

The machine is based on the SENNEBOGEN 870 E base machine with a powerful 261 kW diesel engine. Thanks to the telescoping crawler undercarriage, the 4.2 m and 2.6 m tracks can be adapted. The attachment and the rear ballast can be removed in order to transport the 155 t machine. This reduces the transport weight to 66 t.

**Image caption:**

SENNEBOGEN is showcasing the company's demolition material handler flagship at bauma, the the 870 R-HDD.